Arduino openGLCD Library Version v1.0rc2 |

All Classes Functions Variables Enumerations Enumerator Groups Pages
SED1520
SED1520 based vk5121 panel

The SED1520 uses different timing commands, and control pins than the KS0108 and the most common panels have fewer pixels. The control signals on sed1520 based modules seem to vary substantially from module to module so the distribution contains manual configuration files for a few sed1520 based modules as well as a generic manual configuration file.

- ManualConfig_sed1520-4GLM12232_Panel.h
- ManualConfig_sed1520-mt12232d_Panel.h
- ManualConfig_sed1520-mtb368_Panel.h
- ManualConfig_sed1520-vk5121_Panel.h
- ManualConfig_sed1520_Panel.h

See the individual configuration files for how to hook up the panel.

Note
  Manual configuration files are different from auto configuration files in that they do not auto configure the pins based on board or processor type.